{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["Infrastruct","Ad-hoc"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Infrastruct","index":0,"n_rows":68,"n_cols":14,"rows_kept":68,"cut":false,"hidden":false,"merged":[[19,11,19,12],[51,9,51,10],[51,11,51,12],[52,1,52,2],[51,1,51,2],[51,3,51,4],[51,5,51,6],[51,7,51,8],[19,3,19,4],[19,5,19,6],[19,7,19,8],[19,9,19,10],[20,1,20,2],[3,1,3,2],[4,1,4,2],[3,11,3,12],[3,3,3,4],[3,5,3,6],[3,7,3,8],[3,9,3,10],[5,5,10,8],[19,1,19,2],[36,1,36,2],[35,1,35,2],[35,3,35,4],[35,5,35,6],[21,5,26,8],[37,5,42,8],[53,5,58,8],[21,9,28,12],[53,9,60,12],[35,9,35,10],[35,11,35,12],[35,7,35,8]],"flags":["formulas_cached_only"]}
[]
[null,null,"Ralink3572",null,"802.11n"]
[]
[null,"Infrastruct",null,"Ralink",null,"BCM(610N)",null,"BCM(320N)",null,"DIR-655",null,"IPTIME",null,"comment"]
[null,"2.4 GHz",null,"Up","Down","Up","Down","Up","Down","Up","Down","Up","Down"]
[null,"Ch 1","Mean",14.9,26.9,"채널 수동 선택 지원 안함",null,null,null,15,28.2,14.8,26.7]
[null,null,"Max",15,27.3,{"$nulls":4},15.6,28.9,14.9,27.1]
[null,"Ch 6","Mean",14.8,27,{"$nulls":4},15.2,26.3,14.4,22.3]
[null,null,"Max",14.9,27.2,{"$nulls":4},15.7,27.2,14.7,26.4]
[null,"Ch 11","Mean",14.9,27.1,{"$nulls":4},15,26.9,14.3,20.1]
[null,null,"Max",15,27.2,{"$nulls":4},15.3,27.3,16.1,25.7]
[null,"Auto","Mean",14.9,26.8,14.8,26.5,14.8,25.5,15.1,26.5,12.9,22.9]
[null,null,"Max",14.9,27.1,15,28.1,14.9,28.1,15.2,26.9,14.7,27.1]
[]
[null,null,"** DIR-655  test  시 ch6 에서 연결 끊어짐",{"$nulls":4},"** test 할 때 UI동작 안됨",null,null,null,"** Mean : 6회 평균값"]
[]
[]
[null,null,"Ralink3572",null,"802.11n"]
[]
[null,"Infrastruct",null,"Ralink",null,"BCM(610N)",null,"BCM(320N)",null,"DIR-655",null,"IPTIME",null,"comment"]
[null,"5 GHz",null,"Up","Down","Up","Down","Up","Down","Up","Down","Up","Down"]
[null,"Ch 1","Mean",14.7,26.6,"채널 수동 선택 지원 안함",null,null,null,"2.4 GHz 전용"]
[null,null,"Max",14.8,26.8]
[null,"Ch 6","Mean",15,24.8]
[null,null,"Max",15.2,27.3]
[null,"Ch 11","Mean",14.8,26.6]
[null,null,"Max",14.8,26.8]
[null,"Auto","Mean",14.9,25.7,14.9,27.4,15,27.6]
[null,null,"Max",15,26.5,15,27.8,15.1,28.2]
[]
[]
[]
[]
[null,null,"BCM4323",null,"802.11n"]
[]
[null,"Infrastruct",null,"Ralink",null,"BCM(610N)",null,"BCM(320N)",null,"DIR-655",null,"IPTIME",null,"comment"]
[null,"2.4 GHz",null,"Up","Down","Up","Down","Up","Down","Up","Down","Up","Down"]
[null,"Ch 1","Mean",2.82,4.13,"채널 수동 선택 지원 안함",null,null,null,2.93,4.01,0.68,3.48]
[null,null,"Max",3.26,4.56,{"$nulls":4},3.76,4.09,0.74,4.23]
[null,"Ch 6","Mean",2.3,3.48,{"$nulls":4},2.28,3.09,0.93,2.17]
[null,null,"Max",3.32,4.46,{"$nulls":4},2.88,4.1,2.18,2.87]
[null,"Ch 11","Mean",2.36,4.28,{"$nulls":4},1.87,4.41,0.88,2.4]
[null,null,"Max",3.27,4.5,{"$nulls":4},2.65,5.65,1.72,3.06]
[null,"Auto","Mean",0.93,3.45,3.69,3.62,1.99,2.92,2.16,4.65,0.61,3.03]
[null,null,"Max",1.45,4.08,3.86,4.89,2.14,3.19,3.22,4.72,0.69,3.83]
[]
[null,null,null,"** test 할 때 UI 동작 가능"]
[]
[]
[null,null,"BCM4323",null,"802.11n"]
[]
[null,"Infrastruct",null,"Ralink",null,"BCM(610N)",null,"BCM(320N)",null,"DIR-655",null,"IPTIME",null,"comment"]
[null,"5 GHz",null,"Up","Down","Up","Down","Up","Down","Up","Down","Up","Down"]
[null,"Ch 1","Mean",0.8,2.86,"채널 수동 선택 지원 안함",null,null,null,"2.4 GHz 전용"]
[null,null,"Max",1.03,3.6]
[null,"Ch 6","Mean",1.05,3.55]
[null,null,"Max",1.13,4.28]
[null,"Ch 11","Mean",0.84,3.57]
[null,null,"Max",1.28,4.01]
[null,"Auto","Mean",0.85,3.04,2.76,3.5,3.03,3.78]
[null,null,"Max",1.44,4.14,2.91,4.84,3.32,4.83]
[]
[]
[]
[null,null,"RTL8192SU",null,"802.11n"]
[]
[null,null,"UP",12]
[null,null,"DOWN",1.08]

{"sheet":"Ad-hoc","index":1,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":false,"merged":[[3,2,3,3],[3,4,3,5],[3,6,3,7],[3,8,3,9],[12,2,12,3],[12,4,12,5],[12,6,12,7],[12,8,12,9]],"flags":["formulas_cached_only"]}
[]
[null,"Ralink3572"]
[]
[null,"Ad-hoc","PC 내장",null,"Ralink",null,"BCM",null,"Realtek "]
[null,null,"Up","Down","Up","Down","Up","Down","Up","Down"]
[null,"Mean",null,null,14.5,25.7,4.87,5.12,8.48,3.73]
[null,"Max",null,null,14.6,26.4,5.26,5.68,9.04,4.06]
[null,null,"안됨",{"$nulls":5},"11g"]
[]
[]
[null,"BCM4323"]
[]
[null,"Ad-hoc","PC 내장",null,"Ralink",null,"BCM",null,"Realtek "]
[null,null,"Up","Down","Up","Down","Up","Down","Up","Down"]
[null,"Mean",null,null,0.9,1.42,0.92,1.35,0.9,1.42]
[null,"Max",null,null,1.07,1.48,1.08,1.44,1,1.61]
[null,null,"안됨",{"$nulls":5},"11g"]